For 1990-2009 cars

The PG starter motors are non-repairable starter motors. They have pole pieces that are arranged around the armature. Both solenoid windings are energized. The pull-in winding circuit is completed to the ground through the starter motor. The windings work together magnetically to pull and hold in the plunger. The plunger moves the shift lever. This action causes the starter drive assembly to rotate on the armature shaft spline as it engages with the flywheel ring gear on the engine. Moving at the same time, the plunger also closes the solenoid switch contacts in the starter solenoid. Full battery voltage is applied directly to the starter motor and it cranks the engine.

As soon as the solenoid switch contacts close, current stops flowing thorough the pull-in winding because battery voltage is applied to both ends of the windings. The hold-in winding remains energized. Its magnetic field is strong enough to hold the plunger, shift lever, starter drive assembly, and solenoid switch contacts in place to continue cranking the engine. When the engine starts, pinion overrun protects the armature from excessive speed until the switch is opened.

When the ignition switch is released from the START position, the START relay opens and battery voltage is removed from the starter solenoid S terminal. Current flows from the motor contacts through both windings to the ground at the end of the hold-in winding. However, the direction of the current flow through the pull-in winding is now opposite the direction of the current flow when the winding was first energized.

The magnetic fields of the pull-in and hold-in windings now oppose one another. This action of the windings, along with the help of the return spring, causes the starter drive assembly to disengage and the solenoid switch contacts to open simultaneously. As soon as the contacts open, the starter circuit is turned OFF.

### Circuit Description

Moving the ignition switch to the START position signals the body control module (BCM) through discrete inputs from the ignition transducer that engine crank has been requested. The BCM verifies that theft is not active and sends a serial data message to the engine control module (ECM)/powertrain control module (PCM) requesting engine start. The ECM/PCM receives a 12-volt signal from the park/neutral position (PNP) switch or clutch pedal start switch notifying that it is safe to start the engine. There is a splice on this circuit in the fuse block-underhood that supplies power for the starter relay coil. The starter relay coil control circuit is then grounded by the ECM/PCM closing the switch in the starter relay suppling 12 volts to the S-terminal of the starter. Ground is supplied through the engine block.