For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Ground Nut | 20 N·m | 15 lb ft
Battery Retainer Bolt | 18 N·m | 13 lb ft
Engine Harness Ground Nut | 17 N·m | 13 lb ft
Engine Harness Ground Stud | 25 N·m | 18 lb ft
Generator Bolt (RPO LSJ) | 25 N·m | 18 lb ft
Generator Bolt (RPOs L61/LE5) | 22 N·m | 16 lb ft
Generator Terminal Nut | 20 N·m | 15 lb ft
Junction Block Nut | 17 N·m | 13 lb ft
Negative Battery Cable Bolt | 17 N·m | 13 lb ft
Positive Battery Cable Bolt | 17 N·m | 13 lb ft
Starter Motor Bolt (RPO LSJ) | 50 N·m | 37 lb ft
Starter Motor Bolt (RPOs L61/LE5) | 40 N·m | 30 lb ft
Starter Solenoid Terminal Nut (RPO LSJ) | 11 N·m | 97 lb in
Starter Solenoid Terminal Nut (RPOs L61/LE5) | 17 N·m | 13 lb ft
Starter Solenoid S Terminal Nut | 3 N·m | 27 lb in