For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Remove the oil level indicator.
3. Remove the engine harness clip (2) from the oil level indicator tube bracket.
4. Remove the air conditioning (A/C) compressor/condenser line clip (1) from the oil level indicator tube bracket.
5. Remove the oil level indicator tube bolt.
6. Remove the oil level indicator tube.
7. Remove the oil level indicator tube O-ring seals, if necessary.

### Installation Procedure

1. Install NEW oil level indicator tube O-ring seals, if necessary.
2. Install the oil level indicator tube.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil level indicator tube bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

4. Install the A/C compressor/condenser line clip (1) to the oil level indicator tube bracket.
5. Install the engine harness clip (1) to the oil level indicator tube bracket.
6. Install the oil level indicator.
7. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement .