For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Fender Nameplate

#### Procedure

1. When removing protective liners from adhesive backed nameplates, be careful not to touch the tape with hands and do not allow the tape to come in contact with dirt or any foreign matter prior to adhesion.
2. Use a J 25070 or equivalent to remove the old nameplate.
3. Using a 50/50 solution by volume of isopropyl alcohol and clean drinkable water, clean all the adhesive residue from the fender.
4. Wipe the surface dry with a clean lint-free towel prior to installing new GM nameplate.
5. Press the nameplate firmly to the fender to ensure full adhesion is made to the fender.

#### Special Tools

J 25070 Heat Gun 500-750°F