For 1990-2009 cars

### Removal Procedure

1. Cycle the sunroof window to the partially open position.
2. Pull downward on the sunshade. Cycle the sunroof to full open position. Disengage the sunshade from the sunroof glass panel.
3. Depress the panel (2) to one side of the track assembly.
4. Carefully arch the sunshade upward at the forward center edge.
5. Carefully lift the front edge (1) of the sunshade upward out of the track.
6. Slightly rotate the sunshade panel in order to remove the panel from the track assembly.
7. Carefully remove the sunshade panel upward from the sunroof module.

### Installation Procedure

1. Position rear edge of the sunshade panel to the track assembly.
2. Ensure that the slider pad at the rear is positioned into the track assembly.
3. Depress the rear slider pad on the opposite side of the sunshade panel and release it into the track assembly.
4. Install the front edge (1) of the sunshade panel slider pad into the track assembly.
5. Arch the forward edge of the sunshade in order to insert it into sunshade track.
6. Install the slider pad into the track assembly and release.
7. Slide the sunshade panel forward and rearward to ensure free operation is present.
8. With the sunshade partially open, pull downward on the sunshade. Cycle the sunroof to the vent position, allowing the glass panel to travel past the sunshade front edge.
9. Release the sunshade. Cycle the sunroof to the open position. Inspect for proper engagement of the sunroof glass panel and the sunshade panel.