For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

Notice: Apply pressure only at the end of the liftgate/hood assist rod that you are removing or attaching. Do NOT apply pressure to the middle of the rod because damage or bending will result.

1. Raise and support the hood.
2. Release the hood assist rod upper and lower retainer using a small flat-bladed tool.
3. Remove the hood assist rod (1) from the vehicle.

### Installation Procedure

1. Press the hood assist rod (1) to the upper hood assist rod ball stud until fully seated.
2. Press the hood assist rod (1) onto the lower hood assist rod ball stud until fully seated.
3. Close the hood.