For 1990-2009 cars

### Removal Procedure

1. Disconnect the vehicle speed sensor (VSS) electrical connector.
2. Remove the retainer bolt.
3. Remove the retainer.
4. Pull up on the VSS in order to remove the VSS from the transaxle.
5. Remove the O-ring.

### Installation Procedure

1. Lubricate a new O-ring with DEXRON III transmission fluid.
2. Install the new O-ring.
3. Install the VSS assembly.
4. Install the VSS retainer.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the VSS retainer bolt.

Tighten
Tighten the bolt to 12 N·m (8 lb ft).

6. Connect the VSS connector to the VSS.
7. Lower the vehicle.