For 1990-2009 cars

## Clutch Master Cylinder Replacement M86

### Removal Procedure

1. Remove the clutch pedal retainer from the front of the clutch pedal assembly.
2. Pull the clutch pedal upward in order to disengage the clutch master cylinder pushrod from the clutch pedal.
3. Remove the UBEC. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

4. Place a shop towel under the clutch master cylinder in order to catch any fluid loss.
5. Disconnect the clutch hose (1) from the clutch master cylinder.
6. Disconnect the clutch line (2) from the clutch master cylinder.
7. Cap the reservoir and hydraulic lines in order to prevent fluid loss and contamination.
8. Rotate the clutch master cylinder one ¼ turn clockwise and remove the cylinder from the vehicle.

### Installation Procedure

Important: While installing, ensure that the clutch master cylinder pushrod is aligned with he clutch pedal.

1. Install the clutch master cylinder while rotating ¼ turn counterclockwise.
2. Uncap the reservoir and hydraulic lines.
3. Connect the clutch line (2) to the clutch master cylinder.
4. Connect the clutch hose (1) to the clutch master cylinder.
5. Install the UBEC. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
6. Connect the clutch master cylinder pushrod to the clutch pedal.
7. Install the clutch pedal retainer.
8. Bleed the clutch hydraulic system. Refer to Hydraulic Clutch Bleeding .

## Clutch Master Cylinder Replacement MU3

### Removal Procedure

1. Remove the clutch pedal retainer from the front of the clutch pedal assembly.
2. Pull the clutch pedal upward in order to disengage the clutch master cylinder pushrod from the clutch pedal.
3. Remove the UBEC. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

4. Place a shop towel under the clutch master cylinder in order to catch any fluid loss.
5. Disconnect the clutch hose (1) from the clutch master cylinder.
6. Disconnect the clutch line (2) from the clutch master cylinder.
7. Cap the reservoir and hydraulic lines in order to prevent fluid loss and contamination.
8. Rotate the clutch master cylinder one ¼ turn clockwise and remove the cylinder from the vehicle.

### Installation Procedure

Important: While installing, ensure that the clutch master cylinder pushrod is aligned with he clutch pedal.

1. Install the clutch master cylinder while rotating ¼ turn counterclockwise.
2. Uncap the reservoir and hydraulic lines.
3. Connect the clutch line (2) to the clutch master cylinder.
4. Connect the clutch hose (1) to the clutch master cylinder.
5. Install the UBEC. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
6. Connect the clutch master cylinder pushrod to the clutch pedal.
7. Install the clutch pedal retainer.
8. Bleed the clutch hydraulic system. Refer to Hydraulic Clutch Bleeding .