For 1990-2009 cars

## Seat Belt Retractor Pretensioner Replacement - Front Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disable the SIR in Zones 2 or 6. Refer to SIR Disabling and Enabling.

1 | Seat Belt Anchor Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Move the seat to the full forward position to gain access to the bolt. Tighten
45 N·m (33 lb ft)

2 | Seat Belt Adjuster Cover
3 | Seat Belt Adjuster Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Retractor Bolt Tip Remove the center pillar lower trim panel to gain access to the bolt. Refer to Center Pillar Lower Garnish Molding Replacement. Tighten 45 N·m (33 lb ft)
5 | Front Seat Belt Retractor Assembly Tip Disconnect the belt tension sensor electrical connector.