For 1990-2009 cars

## Engine Coolant Thermostat Housing Replacement L61

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Drain the cooling system. Refer to Cooling System Draining and Filling .

Important: A drain has been provided at the bottom of the water pump for engine block coolant drainage.

3. Drain the coolant from the engine block at the water pump drain. After the coolant has drained, tighten the drain bolt.
4. Lower the vehicle.
5. If equipped with a automatic transaxle, perform the following steps, disconnect the engine coolant temperature (ECT) sensor electrical connector (3).
6. Remove the heated oxygen sensor (HO2S) electrical connector clip from the thermostat housing.
7. If equipped with a manual transaxle, disconnect the ECT sensor electrical connector (3).
8. Remove the ECT sensor, if necessary.
9. Reposition the radiator outlet hose clamp (1) at the thermostat cover.
10. Remove the radiator outlet hose from the thermostat cover.
11. Remove the exhaust heat shield studs (2).
12. Remove the exhaust heat shield (1).
13. Reposition the heater inlet and outlet hose clamps at the thermostat housing pipes.
14. Disconnect the heater inlet and outlet hoses (1, 2) from the thermostat housing pipes.
15. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
16. Remove the thermostat housing bolts.

Important: Twist the water transfer pipe while pulling in order to remove it from the water pump.

17. Remove the thermostat from the vehicle.
18. Remove the water transfer pipe from the thermostat housing, if necessary.
19. Remove and discard the water transfer pipe O-ring seals, if necessary.
20. Remove the thermostat cover bolts and cover, if necessary.
21. Remove the thermostat, if necessary.
22. Remove and discard the thermostat cover O-ring seal, if necessary.
23. Remove all debris and thread sealant from the ECT sensor and bolt holes if the housing is being re-used.

### Installation Procedure

1. Install a NEW thermostat cover O-ring seal into the recess groove.
2. Install the thermostat, if necessary.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the thermostat cover bolts, if necessary.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install a NEW thermostat housing to engine gasket onto the thermostat housing.
5. Load the thermostat housing assembly into position.

Important: The water feed pipe seals can be lightly lubricated with coolant to aid during installation.

6. Install NEW O-ring seals onto the water feed pipe.

Important: Lubricate the O-rings with coolant ONLY.

7. Install the water feed pipe into the thermostat housing aligning locator tab.
8. Align the water pipe to water pump.
9. Seat the water feed O-ring seal by pushing inward toward the water pump. Take care not to tear or damage the O-ring.
10. Position the thermostat housing against the engine.
11. Install the thermostat housing bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

12. Lower the vehicle.
13. Connect the heater inlet and outlet hoses (1, 2) to the thermostat housing pipes.
14. Position the heater inlet and outlet hose clamps at the thermostat housing pipes.
15. Install the exhaust heat shield (1).
16. Install the exhaust heat shield studs (2).

Tighten
Tighten the studs to 22 N·m (16 lb ft).

17. Install the radiator outlet hose to the thermostat cover.
18. Position the radiator outlet hose clamp (1) at the thermostat cover.
19. If reinstalling the old sensor, coat the threads with sealant. Refer to Adhesives, Fluids, Lubricants, and Sealers .
20. Install the ECT sensor, if necessary.

Tighten
Tighten the sensor to 20 N·m (15 lb ft).

21. If equipped with a manual transaxle, connect the ECT sensor electrical connector (3).
22. If equipped with an automatic transaxle, perform the following steps, connect the ECT sensor electrical connector (3).
23. Connect the HO2S electrical connector clip to the thermostat housing.

Important: The vehicle must be level when filling the cooling system.

24. Verify the drain valves at the radiator and water pump are closed.
25. Lower the vehicle.
26. Fill the cooling system. Refer to Cooling System Draining and Filling .
27. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement .

## Engine Coolant Thermostat Housing Replacement LE5

### Removal Procedure

1. Remove the intake manifold cover. Refer to Intake Manifold Cover Replacement .
2. Drain the cooling system. Refer to Cooling System Draining and Filling .

Important: A drain has been provided at the bottom of the water pump for engine block coolant drainage.

3. Drain the coolant from the engine block at the water pump drain. After the coolant has drained, tighten the drain bolt.
4. Lower the vehicle.
5. For access, reposition the underhood electrical center/junction block bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
6. If equipped with a automatic transaxle, perform the following steps, disconnect the engine coolant temperature (ECT) sensor electrical connector (3).
7. Remove the heated oxygen sensor (HO2S) electrical connector clip from the thermostat housing.
8. If equipped with a manual transaxle, disconnect the ECT sensor electrical connector (3).
9. Remove the ECT sensor, if necessary.
10. Reposition the radiator surge tank outlet hose clamp (1) at the thermostat cover.
11. Reposition the radiator surge tank outlet hose clamp (2) at the oil cooler.
12. Remove the radiator surge tank outlet hose from the thermostat cover and oil cooler.
13. Reposition the radiator outlet hose clamp (1) at the thermostat housing.
14. Remove the radiator outlet hose from the thermostat housing.
15. Reposition the radiator outlet hose clamp (1) at the thermostat cover.
16. Remove the radiator outlet hose from the thermostat cover.
17. Remove the exhaust heat shield studs (2).
18. Remove the exhaust heat shield (1).
19. Reposition the heater inlet and outlet hose clamps at the thermostat housing pipes.
20. Disconnect the heater inlet (2) and outlet (1) hoses from the thermostat housing pipes.
21. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
22. Remove the thermostat housing bolts.

Important: Twist the water transfer pipe while pulling in order to remove it from the water pump.

23. Remove the thermostat from the vehicle.
24. Remove the water transfer pipe from the thermostat housing, if necessary.
25. Remove and discard the water transfer pipe O-ring seals, if necessary.
26. Remove the thermostat cover bolts and cover, if necessary.
27. Remove the thermostat, if necessary.
28. Remove and discard the thermostat cover O-ring seal, if necessary.
29. Remove all debris and thread sealant from the ECT sensor and bolt holes if the housing is being re-used.

### Installation Procedure

1. Install a NEW thermostat cover O-ring seal into the recess groove.
2. Install the thermostat, if necessary.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the thermostat cover bolts, if necessary.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install a NEW thermostat housing to engine gasket onto the thermostat housing.
5. Load the thermostat housing assembly into position.

Important: The water feed pipe seals can be lightly lubricated with coolant to aid during installation.

6. Install NEW O-ring seals onto the water feed pipe.

Important: Lubricate the O-rings with coolant ONLY.

7. Install the water feed pipe into the thermostat housing aligning locator tab.
8. Align the water pipe to water pump.
9. Seat the water feed O-ring seal by pushing inward toward the water pump. Take care not to tear or damage the O-ring.
10. Position the thermostat housing against the engine.
11. Install the thermostat housing bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

12. Lower the vehicle.
13. Connect the heater inlet (2) and outlet (1) hoses to the thermostat housing pipes.
14. Position the heater inlet and outlet hose clamps at the thermostat housing pipes.
15. Install the exhaust heat shield (1).
16. Install the exhaust heat shield studs (2).

Tighten
Tighten the studs to 22 N·m (16 lb ft).

17. Install the radiator outlet hose to the thermostat cover.
18. Reposition the radiator outlet hose clamp (1) at the thermostat cover.
19. Install the radiator outlet hose to the thermostat housing.
20. Position the radiator outlet hose clamp (1) at the thermostat housing.
21. Install the radiator surge tank outlet hose to the thermostat cover and oil cooler.
22. Position the radiator surge tank outlet hose clamp (2) at the oil cooler.
23. Position the radiator surge tank outlet hose clamp (1) at the thermostat cover.
24. If reinstalling the old sensor, coat the threads with sealant. Refer to Adhesives, Fluids, Lubricants, and Sealers .
25. Install the ECT sensor, if necessary.

Tighten
Tighten the sensor to 20 N·m (15 lb ft).

26. If equipped with a manual transaxle, connect the ECT sensor electrical connector (3).
27. If equipped with a automatic transaxle, perform the following steps, connect the ECT sensor electrical connector (3).
28. Connect the HO2S electrical connector clip to the thermostat housing.

Important: The vehicle must be level when filling the cooling system.

29. Verify the drain valves at the radiator and water pump are closed.
30. Lower the vehicle.
31. Position the underhood electrical center/junction block bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
32. Fill the cooling system. Refer to Cooling System Draining and Filling .
33. Install the intake manifold cover. Refer to Intake Manifold Cover Replacement .

## Engine Coolant Thermostat Housing Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Partially drain the coolant system. Refer to Cooling System Draining and Filling.
2. Remove the thermostat. Refer to Engine Coolant Thermostat Replacement.
3. Disconnect the inlet and outlet heater hoses. Refer to Heater Inlet Hose Replacement and Heater Outlet Hose Replacement.
4. Remove the turbocharger coolant return pipe. Refer to Turbocharger Coolant Return Pipe Replacement.

Note: If replacing the engine coolant thermostat housing, transfer the coolant temperature sensor. Refer to Engine Coolant Temperature Sensor Replacement.

5. Disconnect the coolant temperature sensor harness connector.

1 | Thermostat Housing Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Thermostat Housing
3 | Water Inlet Seal

#### Procedure

Use a new seal.