For 1990-2009 cars

### Removal Procedure

1. Remove the engine cover.
2. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
3. Disconnect the engine fuel feed pipe from the chassis fuel flex hose. Refer to Metal Collar Quick Connect Fitting Service .
4. Use a back up wrench on the fuel rail and disconnect the fuel feed pipe.
5. Remove the fuel feed pipe fastener located on the engine.
6. Remove the engine fuel feed pipe.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the fuel feed pipe to the fuel rail.

Tighten
Using a backup wrench on the fuel rail tighten the fuel feed pipe to 14 N·m (10 lb ft).

2. Install the engine fuel feed pipe fastener located on the engine.

Tighten
Tighten the fuel feed pipe fastener to 10 N·m (89 lb in).

3. Connect the engine fuel feed pipe to the chassis fuel flex hose. Refer to Metal Collar Quick Connect Fitting Service .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
5. Inspect for leaks using the following procedure:

5.1. | With the engine OFF, turn ON the ignition for 2 seconds.

5.2. | Inspect for fuel leaks.

5.3. | Turn the ignition OFF.

5.4. | With the engine OFF, turn ON the ignition for 2 seconds.

5.5. | Inspect for fuel leaks.

5.6. | Turn the ignition OFF.

6. Install the engine cover and nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).