For 1990-2009 cars

## Stabilizer Shaft Insulator Replacement FE5

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Stabilizer Shaft Clamp Bolt Tighten 50 N·m (37 lb ft)
2 | Front Stabilizer Shaft Clamp Nut Tighten 50 N·m (37 lb ft)
3 | Front Stabilizer Shaft Clamp
4 | Front Stabilizer Shaft Insulator Tip Place the cut line of the insulator facing the rear of the vehicle.

## Stabilizer Shaft Insulator Replacement FE1/FE3

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheels. Refer to Tire and Wheel Removal and Installation .
3. Remove the stabilizer shaft mounting clamp bolts and clamps from both sides of the vehicle.
4. Remove the bushings from the stabilizer shaft.

### Installation Procedure

1. Install the stabilizer bushings on the stabilizer shaft with the cut line facing rearward.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer shaft clamps and bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the front wheels. Refer to Tire and Wheel Removal and Installation.
4. Lower the vehicle.