For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Lift and support vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Front Wheelhouse Liner Retainer (Qty: 5)
2 | Front Wheelhouse Liner Fastener (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Rocker Panel Screw Tighten 1.5 N·m (13 lb in)
4 | Front Fender Liner Tip Lift the fender liner from the rocker molding.