For 1990-2009 cars

The floor console fuse block is located on the passenger side of the floor console behind the forward panel. The panel has three clips. Pull the panel to disconnect the three clips, and access the fuses. Use the fuse puller to remove fuses.

Fuses | Usage
--- | ---
1 | Fuse Puller
2 | Empty
3 | Empty
4 | Empty
5 | Empty
6 | Amplifier
7 | Cluster
8 | Ignition Switch, PASS-Key® III+
9 | Stoplamp
10 | Heating, Ventilation, Air Conditioning, PASS-Key® III+
11 | Empty
12 | Spare
13 | Airbag
14 | Spare
15 | Windshield Wiper
16 | Climate Control System, Ignition
17 | Window Retained Accessory Power
18 | Empty
19 | Electric Power Steering, Steering Wheel Control
20 | Sunroof
21 | Spare
22 | Empty
23 | Audio System
24 | XM Radio™, OnStar™
25 | Engine Control Module, Transmission Control Module
26 | Door Locks
27 | Interior Lights
28 | Steering Wheel Control Illumination
29 | Power Windows

Relays | Usage
--- | ---
30 | Climate Control System
31 | Empty
32 | Retained Accessory Power (RAP)