For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seats. Refer to Front Seat Replacement - Bucket .
2. Remove the floor console. Refer to Front Floor Console Replacement .
3. Remove the front carpet retainer. Refer to Front Carpet Retainer Replacement .
4. Remove the rear carpet retainer, if equipped. Refer to Rear Carpet Retainer Replacement .
5. Loosen the center lower pillar garnish moldings, if equipped. Refer to Center Pillar Lower Garnish Molding Replacement .
6. Loosen the lower lock pillar garnish moldings, if equipped. Refer to Body Lock Pillar Garnish Lower Molding Replacement .
7. Remove the right rear seat cushion. Refer to Rear Seat Cushion Replacement .
8. Remove the lower front seat belt bolt.

1 | Floor Panel Carpet Assembly