For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Front Stabilizer Shaft Link Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 65 N·m (48 lb ft)
2 | Front Stabilizer Shaft Link