For 1990-2009 cars

#### Special Tools

J 36850 Assembly Lubricant

For equivalent regional tools, refer to Special Tools.

1. Assemble the new accumulator piston seals (30) on the three accumulator pistons (29).
2. Install the 1-2 and 2-3 accumulator assist springs (47, 125).
3. Install the accumulator pistons (29) into the channel plate over the guide pins. The pistons are identical. You can assemble the pistons in any of the three accumulator bores.
4. In order to retain the pistons, apply J 36850 lubricant onto the piston seals.
5. Install the manual valve (800) into channel plate.