For 1990-2009 cars

## Decal or Stripe Replacement Pontiac Front Fender

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the body panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Windshield NA Decal

## Decal or Stripe Replacement Pontiac Front Side Door

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the body panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Front Side Door Upper Decal

## Decal or Stripe Replacement Pontiac Rear Body Side Quarter

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the body panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Body Decal Package

## Decal or Stripe Replacement Chevrolet Hood Panel

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the hood panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Hood Decal

## Decal or Stripe Replacement Chevrolet Roof Panel

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the roof panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Roof Panel Decal

## Decal or Stripe Replacement Chevrolet Coupe Rear Compartment Lid

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the rear compartment lid panel.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | End Gate Upper Stripe
2 | End Gate Lower Stripe

## Decal or Stripe Replacement Chevrolet Rear End Spoiler

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the rear compartment lid spoiler.
2. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

3. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Rear End Spoiler Decal

## Decal or Stripe Replacement Chevrolet Sedan Rear Compartment Lid

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear spoiler assembly. Refer to Rear Spoiler Replacement .
2. Using a J 25070 or equivalent, in a circular motion, remove the old decal from the rear compartment lid.
3. Remove all adhesives as follows:

• | For metal body panels use a 3M Scotch Brite® molding adhesive remover disc, 3M P/N 07502 or equivalent.

• | For plastic panels use a lint-free cloth with Varnish Makers and Painters (VMP) Naptha or a 50/50 mixture, by volume of isopropyl alcohol and clean drinkable water to remove left over adhesive.

4. For the final preparation prior to application of the new decal, refer to Graphics/Decals/Emblems .

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | End Gate Upper Stripe