For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

The GMLAN modules on this vehicle also support DTC Symptom information. Refer to DTC Symptom Description for additional information on DTC Symptoms.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0015 | Left Front Seat Belt Pretensioner Deployment | SDM | DTC B0015
B0016 | Left Roof Rail Deployment Loop | SDM | DTC B0016
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0019 or B0020
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0019 or B0020
B0022 | Right Front Seat Belt Pretensioner Deployment | SDM | DTC B0022
B0023 | Right Roof Rail Deployment Loop | SDM | DTC B0023
B0052 | Deployment Commanded | SDM | DTC B0052 or B0053
B0053 | Deployment Commanded with Loop DTCs present | SDM | DTC B0052 or B0053
B0081 | Passenger Presence System | SDM | DTC B0081
B0083 | Front End Sensor | SDM | DTC B0083
B0085 | Left Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0086 | Right Front Side Impact Sensor | SDM | DTC B0085 or B0086
B0158 | Outside Air Temperature Sensor | BCM | DTC B0158
HVAC | DTC B0158
B0283 | Electric Rear Defrost Circuit | BCM | DTC B0283
B0685 | Security System Indicator Circuit Short to Battery | BCM, IPC | DTC B0685
B1000 | Electronic Control Unit (ECU) Performance | BCM, DRR, IPC, Radio, SDM, VCIM | DTC B1000
B1001 | Option Configuration Error | BCM, DRR, Radio, VCIM | DTC B1001
SDM | DTC B1001
B1004 | Electronic Control Unit Identification Circuit | BCM, DRR, IPC | DTC B1004
B1009 | EEPROM Checksum Mismatch | BCM, Radio | DTC B1009
B1019 | System Configuration Error | SDM | DTC B1019
B1025 | LF Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | RF Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | LR Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | RR Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit | DRR | DTC B1259
B1325 | Device Power 1 Circuit | BCM, IPC, Radio, SDM | DTC B1325
B1370 | Device Ignition 1 Circuit | BCM | DTC B1370
SDM | DTC B1370
B1380 | Device Ignition ACCESSORY Circuit | BCM | DTC B1380
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1441 | Device Ignition OFF, RUN, and CRANK Circuit | BCM | DTC B1441
B1480 | Battery Rundown Protection Circuit | BCM | DTC B1480
B1516 | Battery Current Sensor Performance | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B2455 | Cellular Phone Microphone Circuit Malfunction | OnStar® VCIM | DTC B2455
B2470 | Cellular Phone Antenna Circuit Malfunction | OnStar® VCIM | DTC B2470
B2476 | Cellular Phone Select Service Switch Malfunction | OnStar® VCIM | DTC B2476
B2482 | Cellular Phone Select Switch Range/Performance | OnStar® VCIM | DTC B2482
B2483 | GPS Sensor Circuit Low | OnStar® VCIM | DTC B2483 or B2484
B2484 | GPS Sensor Circuit Open | OnStar® VCIM | DTC B2483 or B2484
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2625 | Display Dimming Pulse Width Modulation (PWM) Output Circuit | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2961 | Key In Ignition Circuit | BCM | DTC B2961
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109 | Keyless Entry Transmitter 1 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3110 | Keyless Entry Transmitter 2 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3111 | Keyless Entry Transmitter 3 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3112 | Keyless Entry Transmitter 4 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3265 | Trunk Release Output Circuit | BCM | DTC B3265
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715, B3716, B3717, B3718, or B3719
B3716 | Front Wiper Relay Drive Circuit Range/Performance | BCM | DTC B3715, B3716, B3717, B3718, or B3719
B3717 | Front Wiper Relay Drive Circuit Low | BCM | DTC B3715, B3716, B3717, B3718, or B3719
B3718 | Front Wiper Relay Drive Circuit High | BCM | DTC B3715, B3716, B3717, B3718, or B3719
B3719 | Front Wiper Relay Drive Circuit Open | BCM | DTC B3715, B3716, B3717, B3718, or B3719
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3903 | Stop Lamp Relay Circuit | BCM | DTC B3903
B3935 | Transponder Authentication Error | TDM | DTC B3935
B3948 | Left Front Turn Signal Circuit | BCM | DTC B3948
B3949 | Right Front Turn Signal Circuit | BCM | DTC B3949
B3950 | Left Rear Turn Signal Circuit | BCM | DTC B3950
B3951 | Right Rear Turn Signal Circuit | BCM | DTC B3951
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
C0000 | Vehicle Speed Information Circuit | PSCM | DTC C0000
C0035 | LF Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | RF Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | LR Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0050 | RR Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0161 | ABS/TCS Brake Switch Circuit | EBCM | DTC C0161
C0176 | System Thermal Error | PSCM | DTC C0176
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0475 | Electric Steering Motor Circuit | PSCM | DTC C0475
C0545 | Steering Wheel Torque Input Sensor | PSCM | DTC C0545
C0550 | Electronic Control Unit (ECU) Performance | EBCM | DTC C0550
C0551 | Option Configuration Error | EBCM | DTC C0551
C0561 | System Disabled Information Stored | EBCM | DTC C0561 or P0856
C0845 | Device Ignition 1 Circuit | PSCM | DTC C0845
C0895 | Device Voltage | PSCM | DTC C0895
C0899 | Device Voltage Low | EBCM | DTC C0899
C0900 | Device Voltage High | EBCM | DTC C0900
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010, P0011, P0013, or P0014
P0011 | Intake Camshaft Position (CMP) System Performance | ECM | DTC P0010, P0011, P0013, or P0014
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit | ECM | DTC P0010, P0011, P0013, or P0014
P0014 | Exhaust Camshaft Position (CMP) System Performance | ECM | DTC P0010, P0011, P0013, or P0014
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation | ECM | DTC P0016 for the 2.2L (L61) engine or DTC P0016 for the 2.4L engine
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation | ECM, PCM | DTC P0017 for the 2.0L engine or DTC P0017 for the 2.4L engine
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM, PCM |

• | DTC P0030 or P0036 for the 2.0L engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine

P0033 | Supercharger Bypass Valve Solenoid Control Circuit | PCM | DTC P0033
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM, PCM |

• | DTC P0030 or P0036 for the 2.0L engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine

P0053 | HO2S Heater Resistance Sensor 1 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0054 | HO2S Heater Resistance Sensor 2 | ECM | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine or DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine
P0068 | Throttle Body Airflow Performance | ECM, PCM |

• | DTC P0068 for the 2.0L engine

• | DTC P0068 or P0121 for the 2.2L (L61) engine

• | DTC P0068 or P0121 for the 2.4L engine

P0069 | Manifold Absolute Pressure - Barometric Pressure Correlation | PCM | DTC P0069
P0096 | Intake Air Temperature (IAT) Sensor 2 Performance | PCM | DTC P0096
P0097 | Intake Air Temp Low Voltage | PCM | DTC P0097
P0098 | Intake Air Temperature (IAT) Sensor 2 Circuit High Voltage | PCM | DTC P0098
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM, PCM |

• | DTC P0101 for the 2.0L engine

• | DTC P0101 or P1101 for the 2.2L (L61) engine

• | DTC P0101 or P1101 for the 2.4L engine

P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM, PCM |

• | DTC P0102 for the 2.0L engine

• | DTC P0102 or P0103 for the 2.2L (L61) engine

• | DTC P0102 or P0103 for the 2.4L engine

P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM, PCM |

• | DTC P0103 for the 2.0L engine

• | DTC P0102 or P0103 for the 2.2L (L61) engine

• | DTC P0102 or P0103 for the 2.4L engine

P0106 | Manifold Absolute Pressure (MAP) Sensor Performance | ECM, PCM |

• | DTC P0106 for the 2.0L engine

• | DTC P0106

• | DTC P0106 for the 2.4L engine

P0107 | Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage | ECM, PCM |

• | DTC P0107 for the 2.0L engine

• | DTC P0107 or P0108 for the 2.2L (L61) engine

• | DTC P0107 or P0108 for the 2.4L engine

P0108 | Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage | ECM, PCM |

• | DTC P0108 for the 2.0L engine

• | DTC P0107 or P0108 for the 2.2L (L61) engine

• | DTC P0107 or P0108 for the 2.4L engine

P0111 | Intake Air Temperature (IAT) Sensor 1 Performance | PCM | DTC P0111
P0112 | Intake Air Temperature (IAT) Sensor 1 Circuit Low Voltage | ECM, PCM |

• | DTC P0112 for the 2.0L engine

• | DTC P0112 or P0113 for the 2.2L (L61) engine

• | DTC P0112 or P0113 for the 2.4L engine

P0113 | Intake Air Temperature (IAT) Sensor 1 Circuit High Voltage | ECM, PCM |

• | DTC P0113 for the 2.0L engine

• | DTC P0112 or P0113 for the 2.2L (L61) engine

• | DTC P0112 or P0113 for the 2.4L engine

P0116 | Engine Coolant Temperature (ECT) Sensor Performance. | ECM, PCM |

• | DTC P0116 for the 2.0L engine

• | DTC P0116 for the 2.2L (L61) engine

• | DTC P0116 for the 2.4L engine

P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM, PCM |

• | DTC P0117 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.2L (L61) engine

• | DTC P0117 or P0118 for the 2.4L engine

P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM, PCM |

• | DTC P0118 for the 2.0L engine

• | DTC P0117 or P0118 for the 2.2L (L61) engine

• | DTC P0117 or P0118 for the 2.4L engine

P0120 | Throttle Position (TP) Sensor 1 Circuit | ECM, PCM |

• | DTC P0120 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0121 | Throttle Position (TP) Sensor 1 Performance | ECM, PCM |

• | DTC P0121 for the 2.0L engine

• | DTC P0068 or P0121 for the 2.2L (L61) engine

• | DTC P0068 or P0121 for the 2.4L engine

P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM, PCM |

• | DTC P0122 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM, PCM |

• | DTC P0123 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0125 | Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control | PCM | DTC P0125 for the 2.0L engine
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulating Temperature | ECM, PCM |

• | DTC P0128 for the 2.0L engine

• | DTC P0128 for the 2.2L (L61) engine

• | DTC P0128 for the 2.4L engine

P0130 | HO2S Circuit Sensor 1 | PCM | DTC P0130 for the 2.0L engine
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM, PCM |

• | DTC P0131 for the 2.0L engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.2L (L61) engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.4L engine

P0132 | HO2S Circuit High Voltage Sensor 1 | ECM, PCM |

• | DTC P0132 for the 2.0L engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.2L (L61) engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.4L engine

P0133 | HO2S Slow Response Sensor 1 | ECM, PCM |

• | DTC P0133 for the 2.0L engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine

P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM, PCM |

• | DTC P0134 for the 2.0L engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine

P0135 | HO2S Heater Performance Sensor 1 | ECM, PCM |

• | DTC P0135 for the 2.0L engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine

P0136 | HO2S Circuit Sensor 2 | PCM | DTC P0136
P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM, PCM |

• | DTC P0137 for the 2.0L engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.2L (L61) engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.4L engine

P0138 | HO2S Circuit High Voltage Sensor 2 | ECM, PCM |

• | DTC P0138 for the 2.0L engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.2L (L61) engine

• | DTC P0131, P0132, P0137, or P0138 for the 2.4L engine

P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM, PCM |

• | DTC P0140 for the 2.0L engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine

P0141 | HO2S Heater Performance Sensor 2 | ECM, PCM |

• | DTC P0141 for the 2.0L engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.2L (L61) engine

• | DTC P0030, P0036, P0053, P0054, P0135, or P0141 for the 2.4L engine

P0171 | Fuel Trim System Lean | ECM, PCM |

• | DTC P0171 for the 2.0L engine

• | DTC P0171 or P0172 for the 2.2L (L61) engine

• | DTC P0171 or P0172 for the 2.4L engine

P0172 | Fuel Trim System Rich | ECM, PCM |

• | DTC P0172 for the 2.0L engine

• | DTC P0171 or P0172 for the 2.2L (L61) engine

• | DTC P0171 or P0172 for the 2.4L engine

P0201 | Injector 1 Control Circuit | ECM, PCM |

• | DTC P0201, P0202, P0203, or P0204 for the 2.0L engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.2L (L61) engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.4L engine

P0202 | Injector 2 Control Circuit | ECM, PCM |

• | DTC P0201, P0202, P0203, or P0204 for the 2.0L engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.2L (L61) engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.4L engine

P0203 | Injector 3 Control Circuit | ECM, PCM |

• | DTC P0201, P0202, P0203, or P0204 for the 2.0L engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.2L (L61) engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.4L engine

P0204 | Injector 4 Control Circuit | ECM, PCM |

• | DTC P0201, P0202, P0203, or P0204 for the 2.0L engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.2L (L61) engine

• | DTC P0201, P0202, P0203, or P0204 for the 2.4L engine

P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0220 | Throttle Position (TP) Sensor 2 Circuit | ECM, PCM |

• | DTC P0220 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM, PCM |

• | DTC P0222 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM, PCM |

• | DTC P0223 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P0230 | Fuel Pump Relay Control Circuit | ECM, PCM |

• | DTC P0230 for the 2.0L engine

• | DTC P0230 for the 2.2L engine

• | DTC P0230 for the 2.4L engine

P023A | Charge Air Cooler (CAC) Coolant Pump Relay Control Circuit | PCM | DTC P023A
P0300 | Engine Misfire Detected | ECM, PCM |

• | DTC P0300 for the 2.0L engine

• | DTC P0300 for the 2.2L (L61) engine

• | DTC P0300 for the 2.4L engine

P0315 | Crankshaft Position (CKP) System Variation Not Learned | ECM, PCM |

• | DTC P0315 for the 2.0L engine

• | DTC P0315 for the 2.2L (L61) engine

• | DTC P0315 for the 2.4L engine

P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324, P0325, P0326, P0327, or P0328
P0325 | Knock Sensor (KS) Circuit | ECM, PCM |

• | DTC P0325 for the 2.0L engine

• | DTC P0325, P0326, P0327, or P0328 for the 2.2L (L61) engine

• | DTC P0324, P0325, P0326, P0327, or P0328

P0326 | Knock Sensor (KS) Performance | ECM, PCM |

• | DTC P0326 for the 2.0L engine

• | DTC P0325, P0326, P0327, or P0328 for the 2.2L (L61) engine

• | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine

P0327 | Knock Sensor (KS) Circuit Low Voltage | ECM, PCM |

• | DTC P0327 for the 2.0L engine

• | DTC P0325, P0326, P0327, or P0328 for the 2.2L (L61) engine

• | DTC P0324, P0325, P0326, P0327, or P0328 for the 2.4L engine

P0328 | Knock Sensor (KS) Circuit High Voltage | ECM | DTC P0325, P0326, P0327, or P0328 for the 2.2L (L61) engine or DTC P0324, P0325, P0326, P0327, or P0328
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM, PCM |

• | DTC P0335 for the 2.0L engine

• | DTC P0335 or P0336 for the 2.2L (L61) engine

• | DTC P0335 or P0336 for the 2.4L engine

P0336 | Crankshaft Position (CKP) Sensor Performance | ECM, PCM |

• | DTC P0336 for the 2.0L engine

• | DTC P0335 or P0336 for the 2.2L (L61) engine

• | DTC P0335 or P0336 for the 2.4L engine

P0340 | Intake Camshaft Position (CMP) Sensor Circuit | ECM, PCM |

• | DTC P0340 for the 2.0L engine

• | DTC P0340 or P0341 for the 2.2L (L61) engine

• | DTC P0340, P0341, P0365, or P0366 for the 2.4L engine

P0341 | Camshaft Position (CMP) Sensor Performance | ECM, PCM |

• | DTC P0341 for the 2.0L engine

• | DTC P0340 or P0341 for the 2.2L (L61) engine

• | DTC P0340, P0341, P0365, or P0366 for the 2.4L engine

P0351 | Ignition Coil 1 Control Circuit | ECM, PCM |

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0354 for the 2.2L (L61) engine

• | DTC P0351-P0354 for the 2.4L engine

P0352 | Ignition Coil 2 Control Circuit | ECM, PCM |

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0354 for the 2.2L (L61) engine

• | DTC P0351-P0354 for the 2.4L engine

P0353 | Ignition Coil 3 Control Circuit | ECM, PCM |

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0354 for the 2.2L (L61) engine

• | DTC P0351-P0354 for the 2.4L engine

P0354 | Ignition Coil 4 Control Circuit | ECM, PCM |

• | DTC P0351-P0354 for the 2.0L engine

• | DTC P0351-P0354 for the 2.2L (L61) engine

• | DTC P0351-P0354 for the 2.4L engine

P0365 | Exhaust Camshaft Position (CMP) Sensor Circuit | ECM | DTC P0340, P0341, P0365, or P0366
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance | ECM | DTC P0340, P0341, P0365, or P0366
P0411 | Secondary Air Injection (AIR) System Incorrect Air Flow Detected | ECM | DTC P0411
P0412 | Secondary Air Injection (AIR) Solenoid Control Circuit | ECM | DTC P0412 or P0418
P0418 | Secondary Air Injection (AIR) Pump Control Circuit | ECM | DTC P0412 or P0418
P0420 | Catalyst System Low Efficiency | ECM, PCM |

• | DTC P0420 for the 2.0L engine

• | DTC P0420 for the 2.2L (L61) engine

• | DTC P0420 for the 2.4L engine

P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM, PCM |

• | DTC P0442 for the 2.0L engine

• | DTC P0442 for the 2.2L (L61) engine

• | DTC P0442 for the 2.4L engine

P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM, PCM |

• | DTC P0443 for the 2.0L engine

• | DTC P0443 or P0449 for the 2.2L (L61) engine

• | DTC P0443 or P0449 for the 2.4L engine

P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM, PCM |

• | DTC P0446 for the 2.0L engine

• | DTC P0446 for the 2.2L (L61) engine

• | DTC P0446 for the 2.4L engine

P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM, PCM |

• | DTC P0449 for the 2.0L engine

• | DTC P0443 or P0449 for the 2.2L (L61) engine

• | DTC P0443 or P0449 for the 2.4L engine

P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM, PCM |

• | DTC P0451 for the 2.0L engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.2L (L61) engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.4L engine

P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM, PCM |

• | DTC P0452 for the 2.0L engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.2L (L61) engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.4L engine

P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM, PCM |

• | DTC P0453 for the 2.0L engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.2L (L61) engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.4L engine

P0454 | Fuel Tank Pressure (FTP) Sensor Intermittent | ECM, PCM |

• | DTC P0454 for the 2.0L engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.2L (L61) engine

• | DTC P0451, P0452, P0453, or P0454 for the 2.4L engine

P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM, PCM |

• | DTC P0455 for the 2.0L engine

• | DTC P0455 for the 2.2L (L61) engine

• | DTC P0455 for the 2.4L engine

P0461 | Fuel Level Sensor Performance | ECM, PCM | DTC P0461
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM, PCM | DTC P0462
P0463 | Fuel Level Sensor Circuit High Voltage | ECM, PCM | DTC P0463
P0464 | Fuel Level Sensor Circuit Intermittent | ECM, PCM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM, PCM | DTC P0480 or P0481
P0481 | Cooling Fan Relay 2 Control Circuit | ECM, PCM | DTC P0480 or P0481
P0496 | Evaporative Emission (EVAP) System Flow During Non-Purge | ECM, PCM |

• | DTC P0496 for the 2.0L engine

• | DTC P0496 for the 2.2L (L61) engine

• | DTC P0496 for the 2.4L engine

P0502 | Vehicle Speed Sensor (VSS) Circuit Low Voltage | ECM, PCM | DTC P0502 for the Getrag 5 Speed transmission or DTC P0502 for the MU3 transaxle
P0503 | Vehicle Speed Sensor (VSS) Circuit Intermittent | ECM, PCM | DTC P0503 for the Getrag 5 Speed transmission or DTC P0503 for the MU3 transaxle
P0506 | Idle Speed Low | ECM, PCM |

• | DTC P0506 for the 2.0L engine

• | DTC P0506 or P0507 for the 2.2L (L61) engine

• | DTC P0506 or P0507 for the 2.4L engine

P0507 | Idle Speed High | ECM, PCM |

• | DTC P0507 for the 2.0L engine

• | DTC P0506 or P0507 for the 2.2L (L61) engine

• | DTC P0506 or P0507 for the 2.4L engine

P0520 | Engine Oil Pressure (EOP) Sensor Circuit | ECM, PCM | DTC P0520
P0532 | (A/C) Air Conditioning Pressure Sensor Circuit Low Voltage | ECM, PCM | DTC P0532 or P0533
P0533 | (A/C) Air Conditioning Pressure Sensor Circuit High Voltage | ECM, PCM | DTC P0532 or P0533
P0562 | System Voltage Low | ECM, PCM | DTC P0562
TCM | DTC P0562
P0563 | System Voltage High | ECM, PCM | DTC P0563
TCM | DTC P0563
P0575 | Cruise Control Switch Signal Circuit | ECM, PCM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601, P0602, P0603, or P0604
P0602 | Control Module Not Programmed | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601, P0602, P0603, or P0604
P0603 | Control Module Long Term Memory Reset | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601, P0602, P0603, or P0604
P0604 | Control Module Random Access Memory (RAM) | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601, P0602, P0603, or P0604
P0606 | Control Module Internal Performance | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

P0607 | Control Module Performance | ECM, PCM |

• | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610 for the 2.0L engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine

• | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine

P060D | Control Module Accelerator Pedal Position (APP) System Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
P0615 | Starter Relay Control Circuit | ECM, PCM | DTC P0615
P0621 | Generator L-Terminal Circuit | ECM, PCM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM, PCM | DTC P0622
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610
Transmission Control Module (TCM) Long Term Memory Performance | TCM | DTC P062F
P0641 | 5-Volt Reference 1 Circuit | ECM, PCM |

• | DTC P0641 for the 2.0L engine

• | DTC P0641 or P0651 for the 2.2L (L61) engine

• | DTC P0641 or P0651 for the 2.4L engine

P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM, PCM | DTC P0645
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM, PCM |

• | DTC P0650 for the 2.0L engine

• | DTC P0650 for the 2.2L (L61) engine

• | DTC P0650 for the 2.4L engine

P0651 | 5-Volt Reference 2 Circuit | ECM, PCM |

• | DTC P0651 for the 2.0L engine

• | DTC P0641 or P0651 for the 2.2L (L61) engine

• | DTC P0641 or P0651 for the 2.4L engine

P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0689, or P0690 for the 2.2L (L61) engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0689, or P0690 for the 2.2L (L61) engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0689, or P0690 for the 2.2L (L61) engine or DTC P0685, P0689, or P0690 for the 2.4L engine
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700 for the 2.2L (L61) engine or DTC P0700 or P1700 for the 2.4L engine
P0705 | Transmission Range (TR) Switch Circuit | TCM | DTC P0705
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0712
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0713
P0716 | Input Speed Sensor Performance | TCM | DTC P0716
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0717
P0719 | Brake Switch Circuit Low Voltage | ECM, PCM | DTC P0719
TCM | DTC P0719
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0722
P0723 | Output Speed Sensor Circuit Intermittent | TCM | DTC P0723
P0724 | Brake Switch Circuit High Voltage | ECM, PCM | DTC P0724
TCM | DTC P0724
P0741 | Torque Converter Clutch (TCC) System - Stuck Off | TCM | DTC P0741
P0742 | Torque Converter Clutch (TCC) System - Stuck On | TCM | DTC P0742
P0751 | 1-2 Shift Solenoid (SS) Valve Performance - No First or Fourth Gear | TCM | DTC P0751
P0752 | 1-2 Shift Solenoid (SS) Valve Performance - No Second or Third Gear | TCM | DTC P0752
P0756 | 2-3 Shift Solenoid (SS) Valve Performance - No First or Second Gear | TCM | DTC P0756
P0757 | 2-3 Shift Solenoid (SS) Valve Performance - No Third or Fourth Gear | TCM | DTC P0757
P0833 | Clutch Pedal Switch 2 Circuit | ECM, PCM | DTC P0833 for the Getrag 5 Speed Transmission or DTC P0833 for the MU3 transaxle
P0842 | Transmission Fluid Pressure (TFP) Sensor Circuit Low Voltage | TCM | DTC P0842
P0843 | Transmission Fluid Pressure (TFP) Sensor Circuit High Voltage | TCM | DTC P0843
P0856 | Traction Control Torque Request Circuit | ECM | DTC C0561 or P0856
P0961 | Line Pressure Control (PC) Solenoid System Performance | TCM | DTC P0961
P0973 | 1-2 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0973
P0974 | 1-2 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0974
P0976 | 2-3 Shift Solenoid (SS) Control Circuit Low Voltage | TCM | DTC P0976
P0977 | 2-3 Shift Solenoid (SS) Control Circuit High Voltage | TCM | DTC P0977
P1101 | Intake Air Flow System Performance | ECM, PCM |

• | DTC P1101 for the 2.0L engine

• | DTC P0101 or P1101 for the 2.2L (L61) engine

• | DTC P0101 or P1101 for the 2.4L engine

P1133 | HO2S Insufficient Switching Sensor 1 | ECM, PCM |

• | DTC P1133 for the 2.0L engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine

• | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine

P1174 | Fuel Trim Cylinder Balance | ECM | DTC P1174 for the 2.2L (L61) engine or DTC P1174 for the 2.4L engine
P1182 | Supercharger Inlet Pressure Sensor Performance | PCM | DTC P1182
P1183 | Supercharger Inlet Pressure Sensor Circuit Low Voltage | PCM | DTC P1183
P1184 | Supercharger Inlet Pressure Sensor Circuit High Voltage | PCM | DTC P1184
P1258 | Engine Coolant Over Temperature - Fuel Disabled | ECM, PCM | DTC P1258
P1400 | Cold Start Emission Reduction Control System | ECM | DTC P1400 for the 2.2L (L61) engine or DTC P1400 for the 2.4L engine
P1516 | Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance | ECM, PCM |

• | DTC P1516 for the 2.0L engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.2L (L61) engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.4L engine

P1574 | Stop Lamp Switch Circuit | ECM, PCM | DTC P1574
P1629 | Theft Deterrent Fuel Enable Signal Not Received | ECM, PCM | DTC P1629
P1630 | Theft Deterrent Learn Mode Active | ECM, PCM | DTC P1630
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM, PCM | DTC P1631
P1632 | Theft Deterrent Fuel Disable Signal Received | ECM, PCM | DTC P1632
P1668 | Generator L-Terminal Control Circuit | ECM, PCM | DTC P1668
P1680 | Control Module Accelerator Pedal Position (APP) System Performance | PCM | DTC P1680
P1681 | Control Module Throttle Position (TP) System Performance | PCM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060E, P1600, P1621, P1627, P1681, P1683, or P2610
P1682 | Ignition 1 Switch Circuit 2 | ECM, PCM |

• | DTC P1682 for the 2.0L engine

• | DTC P1682 for the 2.2L (L61) engine

• | DTC P1682 for the 2.4L engine

P1810 | Transmission Fluid Pressure (TFP) Position Switch Circuit | TCM | DTC P1810
P1811 | Maximum Adapt and Long Shift | TCM | DTC P1811
P1816 | Transmission Fluid Pressure (TFP) Valve Position Switch Indicates Park/Neutral (P/N) with Drive Ratio | TCM | DTC P1816
P1818 | Transmission Fluid Pressure (TFP) Valve Position Switch Indicates Drive without Drive Ratio | TCM | DTC P1818
P2101 | Control Module Throttle Actuator Position Performance | ECM, PCM |

• | DTC P2101 for the 2.0L engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.2L (L61) engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.4L engine

P2119 | Throttle Closed Position Performance | ECM, PCM |

• | DTC P2119 for the 2.0L engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.2L (L61) engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.4L engine

P2120 | Accelerator Pedal Position (APP) Sensor 1 Circuit | ECM, PCM |

• | DTC P2120 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM, PCM |

• | DTC P2122 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM, PCM |

• | DTC P2123 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2125 | Accelerator Pedal Position (APP) Sensor 2 Circuit | ECM, PCM |

• | DTC P2125 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM, PCM |

• | DTC P2127 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM, PCM |

• | DTC P2128 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2135 | Throttle Position (TP) Sensor 1-2 Correlation | ECM, PCM |

• | DTC P2135 for the 2.0L engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.2L (L61) engine

• | DTC P0120, P0122, P0123, P0220, P0222, P0223, or P2135 for the 2.4L engine

P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM, PCM |

• | DTC P2138 for the 2.0L engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.2L (L61) engine

• | DTC P2120, P2122, P2123, P2125, P2127, P2128, or P2138 for the 2.4L engine

P2176 | Minimum Throttle Position Not Learned | ECM, PCM |

• | DTC P2176 for the 2.0L engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.2L (L61) engine

• | DTC P1516, P2101, P2119, or P2176 for the 2.4L engine

P2227 | Barometric Pressure (BARO) Sensor Performance | PCM | DTC P2227
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | PCM | DTC P2228
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | PCM | DTC P2229
P2430 | Secondary Air Injection (AIR) System Pressure Sensor Circuit | ECM | DTC P2430-P2433
P2431 | Secondary Air Injection (AIR) System Pressure Sensor Performance | ECM | DTC P2430-P2433
P2432 | Secondary Air Injection (AIR) System Pressure Sensor Circuit Low Voltage | ECM | DTC P2430-P2433
P2433 | Secondary Air Injection (AIR) System Pressure Sensor Circuit High Voltage | ECM | DTC P2430-P2433
P2440 | Secondary Air Injection (AIR) System Shut-Off Valve Stuck Open | ECM | DTC P2440
P2444 | Secondary Air Injection (AIR) System Pump Stuck On | ECM | DTC P2444
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534
P2535 | Ignition 1 Switch Circuit High Voltage | ECM, PCM | DTC P2535
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544 for the 2.2L (L61) engine or DTC P2544 for the 2.4L engine
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.2L (L61) engine or DTC P0601, P0602, P0603, P0604, P0606, P0607, P060D, P062F, or P2610 for the 2.4L engine
P2763 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P2763
P2764 | Torque Converter Clutch (TCC) Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P2764
P2A00 | HO2S Circuit Closed Loop (CL) Performance Sensor 1 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine or DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
P2A01 | HO2S Circuit Sensor 2 | ECM | DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.2L (L61) engine or DTC P0133, P0134, P0140, P1133, P2A00, or P2A01 for the 2.4L engine
U0001 | High Speed CAN Communication Bus | PCM | DTC U0001
U0100 | Lost Communication with ECM/PCM | ABS, BCM, TCM | DTC U0100-U0299
U0101 | Lost Communication with TCM | ABS, BCM, ECM, PCM | DTC U0100-U0299
U0107 | Lost Communication with Throttle Actuator Control Module | ECM, PCM | DTC U0100-U0299
U0121 | Lost Communication with Antilock Brake System (ABS) Control Module | BCM, ECM, PCM, TCM | DTC U0100-U0299
U0126 | Lost Communication withPower Steering Control Module (PSCM) | BCM, ECM, PCM | DTC U0100-U0299
U0140 | Lost Communication with Body Control Module (BCM) | RCDLR, VCIM | DTC U0100-U0299
U1300 | Class 2 Data Link Low | PCM | DTC U1300, U1301, or U1305
U1301 | Class 2 Data Link High | PCM | DTC U1300, U1301, or U1305
U1305 | Class 2 Data Link Low or High | PCM | DTC U1300, U1301, or U1305
U2100 | Controller Area Network (CAN) Bus Communication | BCM, EBCM, ECM, IPC, PCM, PSCM, Radio, SDM, TCM, VCIM | DTC U2100
U2103 | Fewer Controllers On Bus Than Programmed | IPC, Radio, SDM, VCIM | DTC U2103
U2105 | Lost Communications with Engine Control System | BCM, EBCM, PSCM, TCM | DTC U2105-U2199
U2106 | Lost Communications with Transmission Control System | BCM, EBCM, ECM | DTC U2105-U2199
U2107 | Lost Communications with Body Control System | EBCM, ECM, IPC, PCM, PSCM | DTC U2105-U2199
U2108 | Lost Communications with ABS/TCS Control System | BCM | DTC U2105-U2199
U2109 | Lost Communications with Powertrain Multiple Control System | EBCM | DTC U2105-U2199
U2111 | Lost Communications with Steering Control System | BCM | DTC U2105-U2199
U2113 | Lost Communications with Sensing Diagnostic Module (SDM) | BCM | DTC U2105-U2199
U2116 | Lost Communications with Instrument Panel Cluster (IPC) | BCM | DTC U2105-U2199
U2125 | Lost Communications with Mobile Communications Control Systems | BCM | DTC U2105-U2199
U2137 | Lost Communications with Vehicle Theft Deterrent (VTD) | BCM | DTC U2105-U2199
U2172 | Lost Communications with Digital Radio Receiver (DRR) | BCM | DTC U2105-U2199
023 | Seat Belt Tension Sensor Circuit Out of Range | PPS | DTC 023
024 | PPS Ignition 1 Voltage Performance | PPS | DTC 024
063 | PPS Out of Calibration | PPS | DTC 063
064 | Communication/ID Performance | PPS | DTC 064
065 | Sensor Circuit Out of Range | PPS | DTC 065