For 1990-2009 cars

## Radiator Outlet Hose Replacement LE5, L61

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Radiator Outlet Hose Assembly Tip

• | Using J 38185 , position the radiator outlet hose clamps aside and remove the hose from the fittings.

• | Note routing of the radiator outlet hose to ensure proper installation.

#### Special Tools

J-38185 Hose Clamp Pliers

## Radiator Outlet Hose Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the underhood electrical junction block bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement

1 | Radiator Outlet Hose Assembly Tip

• | Using J 38185 , position the radiator outlet hose clamps aside and remove the hose from the fittings.

• | Note routing of the radiator outlet hose to ensure proper installation.

#### Special Tools

J-38185 Hose Clamp Pliers