For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the floor console. Refer to Front Floor Console Replacement.
3. Remove the instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.
4. Remove the I/P upper trim pad. Refer to Instrument Panel Upper Trim Panel Replacement.
5. Lower the steering column. Refer to Steering Column Replacement.

1 | Instrument Panel Retainer Assembly Tip Remove the HVAC air ducts.
2 | Instrument Panel Retainer Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
3 | Instrument Panel Retainer Screw (Qty: 17) Tighten 2.2 N·m (20 lb in)
4 | Instrument Panel Retainer Nut (Qty: 8) Tighten 25 N·m (18 lb ft)