For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Loosen the charge air cooler inlet pipe clamp (1).
3. Remove the charge air cooler inlet pipe (2) from the charge air cooler (3).
4. Loosen the charge air cooler clamp (1).
5. Remove the charge air cooler inlet pipe (2) from the vehicle.

### Installation Procedure

Note: Remove any oil film from inside the pipes.

1. Install the charge air cooler pipe (2) and tighten the charge air cooler inlet pipe clamp.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the charge air cooler inlet pipe (2) to the charge air cooler (3) and tighten the clamp to 5 N·m (44 lb in).