For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Remove the brake shoes. Refer to Brake Shoe Replacement.
2. Remove the wheel cylinder. Refer to Wheel Cylinder Replacement.
3. Release the rear park brake cable end fitting (1) from the drum brake backing plate.
4. Remove the rear wheel bearing and hub assembly. Refer to Rear Wheel Bearing and Hub Replacement.
5. Remove the rear brake backing plate from the rear axle assembly.

### Installation Procedure

1. Install the rear brake backing plate to the rear axle assembly.
2. Install the rear wheel bearing and hub assembly. Refer to Rear Wheel Bearing and Hub Replacement.
3. Install the rear park brake cable end fitting (1) to the drum brake backing plate.
4. Install the wheel cylinder. Refer to Wheel Cylinder Replacement.
5. Install the brake shoes. Refer to Brake Shoe Replacement.