For 1990-2009 cars

### Removal Procedure

1. Raise and support the rear compartment lid.
2. Remove the rear compartment hinge bolts (2) from the hinge.
3. Remove the compartment lid hinge nuts (1) from the decklid studs.
4. Remove the compartment lid hinge (3) from the vehicle.

### Installation Procedure

1. Position the rear compartment lid hinge (3) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear compartment hinge nuts (1) to the studs on the decklid.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the rear compartent hinge bolts (2) to the hinge.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Adjust the rear compartment lid if necessary. Refer to Rear Compartment Lid Adjustment.