For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.

1 | Ignition and Start Switch Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Turn the ignition lock cylinder to the run position before removing the ignition and start switch bolts.

Tighten
2 N·m (18 lb in)

2 | Ignition and Start Switch

#### Procedure

1. Disconnect any electrical connectors as needed.
2. If replacing the ignition and start switch, the theft deterrent module must be relearned. Refer to Control Module References.