For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the rear seat back. Refer to Rear Split Folding Seat Back Replacement.
3. Remove the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.

1 | Rear Seat Belt Anchor Bolt - Right Caution: Refer to Fastener Caution in the Preface section. Tighten 45 N·m (33 lb ft)
2 | Rear Seat Belt Retractor Bolt - Right Tighten 45 N·m (33 lb ft)
3 | Rear Seat Belt Retractor Assembly - Right
4 | Rear Seat Belt Anchor Bolt - Center Tighten 45 N·m (33 lb ft)
5 | Rear Seat Belt Retractor Bolt - Center Tighten 45 N·m (33 lb ft)
6 | Rear Seat Belt Retractor Assembly - Center
7 | Rear Seat Belt Anchor Bolt - Left Tighten 45 N·m (33 lb ft)
8 | Rear Seat Belt Retractor Bolt - Left Tighten 45 N·m (33 lb ft)
9 | Rear Seat Belt Retractor Assembly - Left