For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Motor Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Window Regulator Motor Tip Disconnect the electrical connector.