For 1990-2009 cars

1. Ensure that the steering wheel is set in a straight ahead position.
2. Loosen the tie rod jam nut (5).
3. Adjust the toe to specification by turning the adjuster (6). Refer to Wheel Alignment Specifications .

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Tighten the tie rod jam nut (5).

Tighten
Tighten the tie rod jam nut (5) to 68 N·m (50 lb ft).