For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section.

#### Preliminary Procedures

1. Remove the steering column opening filler assembly. Refer to Steering Column Opening Filler Replacement .
2. Tilt the steering wheel up.

1 | Instrument Panel Trim Plate Tip

• | Release the left-hand instrument panel (I/P) trim plate assembly by pulling away from the I/P retainer.

• | Disconnect the electrical connector.

2 | Instrument Panel Trim Plate Clip