For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Caution in the Preface section.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .

1 | Front Side Door Hinge Upper Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Support the door before removing the hinge bolts.
3. Disconnect the electrical connector, if equipped.
4. With the aid of an assistant, remove the door.

Tighten
35 N·m (26 lb ft)

2 | Front Side Door Check Link Bolt Tighten 20 N·m (15 lb ft)
3 | Front Side Door Hinge Lower Bolt (Qty: 2) Tighten 35 N·m (26 lb ft)
4 | Front Side Door Assembly

#### Procedure

When replacing the door it is necessary to transfer all of the internal components.