For 1990-2009 cars

#### Special Tools

• | J 8092 Driver Handle

• | J 41102-1A Axle Seal Installer

For equivalent regional tools, refer to Special Tools.

Note: You must use the J 41102-1A seal installer in order to install the seal correctly. The J 41102-1A seal installer installs the axle seal to a given depth.

1. Install a new side cover axle seal (2) into the side cover. Use the J 41102-1A seal installer with the J 8092 driver handle .
2. In order to prevent damage to the shaft splines during vehicle operation, add Polyurea grease (part number 7843867) to the splines on the output shaft.