For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right front fender liner. Refer to Front Fender Liner Replacement.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Front Intake Air Duct Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Intake Air Duct Retainer
3 | Air Cleaner Inlet Duct Tip Pull the duct straight down.