For 1990-2009 cars

### Removal Procedure

1. Remove the engine oil fill cap.
2. Grasp the intake manifold cover by the lower right inboard corner and pull up to disengage the cover from the stud.
3. Grasp the intake manifold cover by the upper left corner and pull up to disengage the cover from the stud.
4. Remove the intake manifold cover.

### Installation Procedure

1. Place the intake manifold cover onto the engine over the studs.
2. Push down on the intake manifold cover directly over the lower right stud in order to engage the cover to the stud.
3. Push down on the intake manifold cover directly over the upper left stud in order to engage the cover to the stud.
4. Install the engine oil fill cap.