For 1990-2009 cars

## Seat Belt Retractor Pretensioner Replacement - Front Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

Disable the SIR in Zones 2 or 6. Refer to SIR Disabling and Enabling .

1 | Seat Belt Anchor Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Move the seat to the full forward position to gain access to the bolt. Tighten
45 N·m (33 lb ft)

2 | Seat Belt Adjuster Cover
3 | Seat Belt Adjuster Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Retractor Bolt Tip Remove the center pillar lower trim panel to gain access to the bolt. Refer to Center Pillar Lower Garnish Molding Replacement . Tighten 45 N·m (33 lb ft)
5 | Front Seat Belt Retractor Assembly Tip Disconnect the belt tension sensor electrical connector.

## Seat Belt Retractor Pretensioner Replacement - Front Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedures

Disable the SIR. Refer to SIR Disabling and Enabling .

1 | Seat Belt Anchor Bolt Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. Move the seat to the full forward position.
2. Pull the seat belt anchor cover upward to gain access to the bolt.

Tighten
45 N·m (33 lb ft)

2 | Seat Belt Retractor Bolt Tip Remove the body lock pillar lower trim panel to gain access to the bolt. Refer to Body Lock Pillar Garnish Lower Molding Replacement . Tighten 45 N·m (33 lb ft)
3 | Front Seat Belt Guide Screw Tighten 9 N·m (80 lb ft)
4 | Seat Belt Adjuster Bolt Tip Flip open the seat belt adjuster cover to gain access to the bolt. Tighten 45 N·m (33 lb ft)
5 | Front Seat Belt Retractor Assembly

1. Disconnect the belt tension sensor electrical connector.
2. Remove the seat belt assembly from the seat belt guide attached to the head restraint.