For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Drain Plugs | 38 N·m | 28 lb ft
Front Transmission Mount Bolts | 50 N·m | 37 lb ft
Front Transmission Mount Through Bolt | 100 N·m | 74 lb ft
Heat Shield to Engine Block Bolt | 30 N·m | 22 lb ft
Heat Shield to Transmission Mount Bolt | 10 N·m | 89 lb in
Intermediate Shaft Bolt | 100 N·m | 74 lb ft
Rear Cover Bolts | 25 N·m | 18 lb ft
Rear Transmission Mount Bracket to Transmission Bolts | 60 N·m | 44 lb ft
Rear Transmission Mount Through Bolt | 100 N·m | 74 lb ft
Rear Transmission Mount to Frame Bolts | 60 N·m | 44 lb ft
Reverse Lockout Bolt | 6 N·m | 53 lb in
Reverse Switch | 18 N·m | 13 lb ft
Ring Gear | 90 N·m | 66 lb ft
Side Transmission Mount Bolts | 45 N·m | 33 lb ft
Side Transmission Mount to Mid-Rail Bolts | 34 N·m | 25 lb ft
Shaft Bolts | 100 N·m | 74 lb ft
Shift Cable Attachment Nut | 10 N·m | 89 lb in
Shift Control Nuts | 25 N·m | 18 lb ft
Shifter Guide Bolt | 25 N·m | 18 lb ft
Shifter Retaining Bolts | 25 N·m | 18 lb ft
Speed Sensor | 12 N·m | 106 lb in
Transmission Housing Bolts | 27 N·m | 20 lb ft
UBEC Bracket Bolts | 25 N·m | 18 lb ft
UBEC Bracket Nuts | 10 N·m | 89 lb in
UBEC Positive Post | 10 N·m | 89 lb in