For 1990-2009 cars

### Description

The Eaton™ M 62 is a fifth generation Roots™-type supercharger. The supercharger is a positive displacement pump that consists of 2 counter-rotating rotors in a housing with an inlet port and an outlet port. The rotors are designed with 3 lobes and a helical 60° twist from front to back. An air bypass valve is built into the housing. The rotors in the supercharger are designed to run at a minimal clearance, not in contact with each other or the housing. The rotors are timed to each other by a pair of precision spur gears which are pressed onto the rotor shafts. The forward end of the rotors are held in position by deep-groove ball bearings. The back end of the rotors are supported by sealed roller bearings.

The gears and ball bearings are lubricated by a synthetic oil. The oil reservoir is self-contained in the supercharger and does not rely on engine oil for lubrication. This oil reservoir is sealed for the life of the unit and is not serviceable.

The cover on the supercharger contains the input shaft which is supported by 2, deep-groove ball bearings and is coupled to the rotor drive gears. The pulley is pressed onto the input shaft and is not serviceable. These bearings are lubricated by the synthetic oil contained in the same reservoir as the gears and rotor bearings.

### Operation

The supercharger is designed to pump more air than the engine would normally use. This excess air creates a boost pressure in the intake manifold. Maximum engine boost is 83 kPa (12 psi). Because the supercharger is a positive displacement pump and is directly driven from the engine drive belt system, boost pressure is available at all driving conditions.

When boost is not desired, such as during idle and light throttle cruising, the excess air that the supercharger is producing is routed through the bypass passage between the intake manifold and the supercharger inlet. This bypass circuit is regulated by a bypass valve which is similar to a throttle plate. The bypass valve is controlled by a vacuum actuator which is connected to the vacuum signal between the throttle and the supercharger inlet. Spring force from the actuator holds the valve closed to create boost, and vacuum pulls the valve open when the throttle closes to decrease boost. The open bypass valve reduces pumping loss thereby increasing fuel efficiency.

The solenoid valve attached to the bypass actuator is an electronically controlled, 3-way valve. This valve, controlled by the powertrain control module (PCM), determines whether pressure from the manifold is routed to the bypass actuator or closed off. The valve allows pressure from the manifold to open the bypass valve and regulate boost pressure during specific driving conditions.

### Intercooler

The supercharger has an integrated intercooler. Cooling the air enhances the effectiveness of the supercharger. The intercooler uses conventional coolant in a separate sealed system from the engine cooling system. The intercooler system has a radiator, a reserve tank/filler neck, a pressure cap, attaching hoses, and a pump capable of a 26 liters (7 gallons) per minute flow rate. The pump is commanded ON, by the control module, whenever the engine is running.