For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the armrest pull cup. Refer to Armrest Pull Cup Replacement .
2. Remove the manual window regulator handle if equipped. Refer to Door Window Regulator Handle Replacement .
3. Disconnect the inside door handle cable. Refer to Door Inside Handle Replacement .

1 | Screw, Side Door Trim (Qty: 2) Tighten 2.2 N·m (19 lb in)
2 | Panel Assembly, Side Door Trim
3 | Retainer, Side Door Trim