For 1990-2009 cars

#### Special Tools

• | J 41231 Inner Seal Installer

• | J 23327 Return Spring Compressor

For equivalent regional tools, refer to Special Tools.

1. Assemble a new inner seal assembly (608) if the old seal was damaged and removed. Use an arbor press and the J 41231 seal installer in order to press the inner seal assembly onto the forward clutch housing (609).
2. Assemble the forward clutch piston assembly (607) into the forward clutch housing (609). In order to ease assembly, lubricate the seals with transmission fluid.
3. With the snap ring tabs facing up, assemble the forward clutch return spring assembly (606) into the forward clutch housing (609).

Caution: Compress the return spring (606) only enough to install the snap ring (605), or damage may occur to the spring assembly (606).

4. Compress the return spring assembly. Use the J 23327 spring compressor .
5. Assemble the snap ring (605) in order to retain the forward clutch return spring.
6. Remove the J 23327 spring compressor .
7. Install the forward clutch waved plate (604).
8. Install the seven steel plates (603) and the seven new fiber plates (602) in alternating order beginning with a steel plate (603).
9. Install the forward clutch backing plate (601).
10. Install the forward clutch backing plate snap ring (600) in order to retain the clutch pack.