For 1990-2009 cars

#### Special Tools

• | J 28467-B Universal Engine Support Fixture

• | J 28467-500 Engine Support Fixture

### Installation Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
2. Place the engine support fixture legs (1) from the J 28467-B across the engine compartment.
3. Install the engine support fixture legs (1) from the J 28467-500 on the engine support fixture long bar (2).
4. Install the radiator shelf tube J-28467-2A (1) on top of the strut tower tube J-28467-3 (2) above the engine front (right back) lift hook bracket.
5. Install the round tube of the front support assembly J-28467-4A (3) through the large hole in the radiator shelf tube J-28467-2A.
6. Locate the J-28467-4A front support assembly to the upper tie bar.
7. Install the J-28467-9 7/16 inch x 2.0 inch quick-release pin (4) through the top hole in the J-28467-4A front support assembly.
8. Install the J-28467-1A cross bracket assembly (1).
9. Hand tighten the J-28467-1A cross bracket wing nuts (2).
10. Install the J-28467-7A bolt hook through the J-28467-6A bracket.
11. Install the J-28467-34 lift hook wing nut and washer to the J-28467-7A lift hook.
12. Repeat the previous 2 steps in order to assemble 2 lift hooks and brackets.
13. Install one of the lift hook and bracket assemblies (1) to the engine support fixture long bar (2).
14. Install the other lift hook and bracket assembly (3) to the J-28467-2A radiator shelf tube (4) above the engine front lift bracket.
15. Install the lift hook J-28467-7A through the engine rear lift bracket (2).
16. Install the lift hook J-28467-7A (3) through the engine front lift bracket (4).
17. Hand tighten the lift hook wing nuts J-28467-34 (5) in order to remove all slack from the engine support fixture assembly.