For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tip Loosen the bolts enough so that the regulator assembly will lift out of the t-slots in the door inner panel. Tighten
10 N·m (89 lb in)

2 | Rear Side Door Window Regulator Assembly
3 | Rear Side Door Window Regulator Motor Tip Disconnect the electrical connector.