For 1990-2009 cars

Connector 1: | Fuse Holder - 50 AMP
Connector 2: | Ignition Switch

### Fuse Holder - 50 AMP

#### Connector Part Information

- OEM: 12110057
- Service: 12110057
- Description: 2-Way F Maxi (BK)

#### Terminal Part Information

- Terminal/Tray: 12110127/19
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Fuse Holder - 50 AMP

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD/BK | 142 | Battery Positive Voltage
B | RD | 1 | Unfused Battery Positive Voltage

### Ignition Switch

#### Connector Part Information

- OEM: 15324806
- Service: 88987854
- Description: 6-Way F 035 Series ILAG5 (GN)

#### Terminal Part Information

- Terminal/Tray: IL-AG5-C1-5000 /20
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: J-38125-211/J-35616-64B (L-BU)

#### Ignition Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RD/WH | 1040 | Battery Positive Voltage
3 | YE | 5199 | Run/Crank Voltage
4 | BN | 4 | Accessory Voltage
5 | WH | 1390 | Off/Run/Crank Voltage
6 | WH/BK | 1073 | Key-In Ignition Switch