For 1990-2009 cars

#### Tools Required

• | J 38122-A Crankshaft Balancer Holder

• | J 43653 Flywheel Holding Tool

Important: J 43653 may be used instead of J 38122-A to prevent crankshaft rotation.

1. Install the J 38122-A .
2. Remove the balancer retaining bolt and washer. Use the J 38122-A and a breaker bar to prevent the crankshaft from rotating when loosening the bolt.

Discard the bolt.

3. Remove the crankshaft balancer assembly.