For 1990-2009 cars

## Tail/Turn Signal Lamp Replacement Chevrolet Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear compartment trim panel. Refer to Rear Compartment Trim Panel Replacement.
2. Disconnect the electrical connector from the stop/turn signal lamp socket.
3. Remove the stop/turn bulb lamp socket from the lamp assembly.

1 | Tail Turn Signal Lamp Nut (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 5 N·m (44 lb in)
2 | Tail Lamp Turn Signal Lamp Assembly Tip Push the lamp assembly outward from the rear end panel extension.