For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to disengage the clips located at the sides of the switch bezel.
2. Remove the bezel (1) from the headliner.
3. Remove the sunroof control switch (2) from the metal housing in the headliner using a small, flat-bladed tool at the front and rear of the switch.
4. Disconnect the electrical connector from the sunroof control switch.

### Installation Procedure

1. Connect the harness to the switch.
2. Install the sunroof control switch (2) to the metal housing in the headliner.
3. Press the bezel to the headliner to engage the clips.