For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC U0100 00: Lost Communication With ECM/PCM
DTC U0100 75: Lost Communication With ECM/PCM
DTC U0100 7F: Lost Communication With ECM/PCM
DTC U0101 00: Lost Communication With TCM
DTC U0102 00: Lost Communication With Transfer Case Control Module
DTC U0104 00: Lost Communication With Cruise Control Module
DTC U0104 7F: Lost Communication With Cruise Control Module
DTC U0106 00: Lost Communication With Glow Plug Control Module
DTC U0109 00: Lost Communication With Fuel Pump Control Module
DTC U0117 00: Lost Communication With Electrical PTO Control Module
DTC U0121 00: Lost Communication With Anti-Lock Brake System (ABS) Control Module
DTC U0122 00: Lost Communication With Vehicle Dynamics Control Module (ALC/ESC/ASCM)
DTC U0131 00: Lost Communication With Power Steering Control Module
DTC U0132 00: Lost Communication With Ride Level Control Module
DTC U0134 00: Lost Communication With Power Steering Control Module - Rear
DTC U0136 00: Lost Communication With Differential Control Module - Rear
DTC U0140 00: Lost Communication With Body Control Module
DTC U0141 00: Lost Communication With Body Control Module A
DTC U0151 00: Lost Communication With Restraints Control Module
DTC U0151 71: Lost Communication With Restraints Control Module Invalid Serial Data Received
DTC U0151 7F: Lost Communication With Restraints Control Module Erratic
DTC U0155 00: Lost Communication With Instrument Panel Cluster (IPC) Control Module
DTC U0156 00: Lost Communication With Information Center A (DIC)
DTC U0158 00: Lost Communication With Head Up Display
DTC U0159 00: Lost Communication With Parking Assist Control Module
DTC U0160 00: Lost Communication With Audible Alert Control Module
DTC U0164 00: Lost Communication With HVAC Control Module
DTC U0165 00: Lost Communication With HVAC Control Module - Rear
DTC U0168 00: Lost Communication With Vehicle Security Control Module
DTC U0170 00: Lost Communication With Restraints System Sensor A (PPS)
DTC U0172 00: Lost Communication With Rollover Sensor
DTC U0184 00: Lost Communication With Radio
DTC U0186 00: Lost Communication With Audio Amplifier
DTC U0291 00: Lost Communication With Television
DTC U0194 00: Lost Communication With Digital Radio Receiver (DRR)
DTC U0198 00: Lost Communication With Telematic Control Module (VCIM)
DTC U0199 00: Lost Communication With Door Control Module A (DDM)
DTC U0200 00: Lost Communication With Door Control Module B (PDM)
DTC U0208 00: Lost Communication With Seat Control Module A (DSM/MSM)
DTC U0209 00: Lost Communication With Seat Control Module B (HVSM)
DTC U0210 00: Lost Communication With Seat Control Module C (RHVSM)
DTC U0214 00: Lost Communication With Remote Function Actuation
DTC U0230 00: Lost Communication With Rear Gate Module
DTC U0232 00: Lost Communications With Side Object Detection (SOD) Module - Left
DTC U0233 00: Lost Communications With Side Object Detection (SOD) Module - Right
DTC U0236 00: Lost Communications With Column Locking Module (CLM)
DTC U0241 00: Lost Communication With Headlamp Control Module A
DTC U0249 00: Lost Communication With Entertainment Control Module - Rear B

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Module B+ | U0100-U0299 | U0100-U0299 | -- | --
Ignition | U0100-U0299 | U0100-U0299 | -- | --
Module Ground | U0100-U0299 | U0100-U0299 | -- | --
Accessory Wake Up Serial Data | U1814 | U0100-U0299 | -- | --
High Speed GMLAN Serial Data Wake Up | U2099 | U0100-U0299 | -- | --
High Speed GMLAN Serial Data (+) | 2 | U0100-U0299 | 2 | --
High Speed GMLAN Serial Data (-) | 2 | U0100-U0299 | 2 | --
Low Speed GMLAN Serial Data | 1 | U0100-U0299 | 1 | --
1. Scan tool does not communicate with low speed GMLAN device 2. Scan tool does not communicate with high speed GMLAN device

### Circuit/System Description

Modules connected to the high and low speed GMLAN serial data circuits monitor for serial data communications during normal vehicle operation. Operating information and commands are exchanged among the modules.

The body control module (BCM) activates the serial data communication enable and the accessory wakeup serial data circuits by applying voltage when the ignition key is in ACC, ON or START. Only the modules using high speed GMLAN serial data are connected to the enable or wakeup circuits. To determine which modules are activated using the enable or wakeup circuits refer to Data Communication Schematics .

### Conditions for Running the DTC

The system voltage is between 9-16 volts.

### Conditions for Setting the DTC

A supervised periodic message that includes the transmitter module availability has not been received.

### Action Taken When the DTC Sets

Specific subsystems will not function.

### Conditions for Clearing the DTC

• | A current DTC clears when the malfunction is no longer present.

• | A history DTC clears when the module ignition cycle counter reaches the reset threshold of 50, without a repeat of the malfunction.

### Diagnostic Aids

• | Use the DTC Descriptor list above to determine the module which is not communicating.

• | If there are multiple non-communicating modules choose the one closest to the data link connector (DLC).

• | Use Data Link References to determine if the module uses high or low speed GMLAN serial data communications.

• | Some modules may not have internal protection for specific voltage outputs and may open a battery positive voltage or ignition voltage source fuse. If a voltage input fuse is open and no short is found in that circuit, ensure that no module output voltage circuit is shorted to ground before replacing the module.

• | This diagnostic can be used for any module that should communicate with high or low speed GMLAN serial data providing the vehicle is equipped with the option that uses that module.

### Reference Information

#### Schematic Reference

• | Data Communication Schematics

• | Control Module References

#### Connector End View Reference

• | Component Connector End Views

• | Splice Pack Connector End Views

#### Description and Operation

Data Link Communications Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Verify that following BCM DTCs are not present:

• | U1814

• | U2099

• | B1428

• | B1370

• | B1380

• | B1440

• | B1441

⇒ | If any listed DTC is present, refer to Diagnostic Trouble Code (DTC) List - Vehicle to diagnose that DTC prior to this diagnostic.

2. Verify that at least 1 module that communicates on high speed GMLAN serial data communicates with the scan tool.

⇒ | If no module communicates on high speed GMLAN serial data, refer to Scan Tool Does Not Communicate with High Speed GMLAN Device .

3. Verify that at least 1 module, excluding BCM, that communicates on low speed GMLAN serial data communicates with the scan tool.

⇒ | If no module communicates on low speed GMLAN serial data, excluding BCM, refer to Scan Tool Does Not Communicate with Low Speed GMLAN Device .

### Circuit/System Testing

1. Using the DTC Descriptor and Diagnostic Aids above, determine the module that is not communicating.
2. Ignition OFF, disconnect the necessary harness connector of the module that is not communicating.
3. Test for less than 1 ohm between the module ground circuits and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

Important: Only the high speed GMLAN modules have a serial data communication enable circuit OR an accessory wakeup serial data circuit, and the BCM is the output for these circuits. Refer to the module schematics to identify which modules have these circuits. If the module that is not communicating is the BCM or does not have one of these circuits, proceed to step 5.

4. Ignition ON, verify that a test lamp illuminates between the serial data communication enable circuit OR the accessory wakeup serial data circuit and ground.

⇒ | If the test lamp does not illuminate, test the circuit for an open/high resistance. If the circuits test normal, replace the BCM.

5. Ignition ON, verify that a test lamp illuminates between all battery positive voltage circuits and ground.

⇒ | If the test lamp does not illuminate, test the circuit for a short to ground or an open/high resistance. If the circuit fuse is open, also test the positive voltage outputs of the module for a short to ground. If the circuits test normal, replace the module.

6. Verify that a test lamp illuminates between all ignition voltage circuits and ground.

⇒ | If the test lamp does not illuminate, test the circuit for a short to ground or an open/high resistance. If the circuit fuse is open, also test the positive voltage outputs of the module for a short to ground. If the circuits test normal, replace the module.

7. Test for less than 1 ohm on the GMLAN serial data circuits between the non-communicating module and the module that displays the DTC.

⇒ | If greater than the specified range, test the serial data circuit for open/high resistance.

8. If all circuits test normal, replace the module that is not communicating.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | GMLAN Wiring Repairs

• | Control Module References for module replacement, setup, and programming