For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. Please refer to Recommended Fluids and Lubricants for more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer for more information.
Cooling System

- 2.2L and 2.4L Engines

7.4 qt

7.0L

Engine Oil with Filter

- 2.2L L4 and 2.4L L4 Engines

5.0 qt

4.7 L

Fuel Tank

- 2.2L L4 Engine (with NU6 emissions) sold new in CA, ME, VT, NY, NH, MA (see your dealer for bordering states

13.5 gal

51.1 L

- 2.2L L4 Engine (without NU6 emissions) sold new in all other states (see your dealer for more information)

13.0 gal

49.2 L

- 2.4L L4 Engine sold new in all states

13.0 gal

49.2 L

Transaxle, Automatic (Complete Drain and Refill) | 7.0 qt | 6.6 L
Transaxle, Manual (Complete Drain and Refill) | 1.7 qt | 1.6 L
Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the appropriate level, as recommended in this manual.

#### Engine Specifications

Engine | VIN Code | Transaxle | Spark Plug Gap
--- | --- | --- | ---
2.2L L4 | F | Automatic Manual | 0.040 inch (1.01 mm)
2.4L L4 | B | Automatic Manual | 0.040 inch (1.01 mm)