For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Disconnect the inlet and outlet pipes to the charge air cooler. Refer to Charge Air Cooler Inlet Pipe Replacement and Charge Air Cooler Outlet Pipe Replacement .

1 | Charge Air Cooler Bolt (Qty:4) Notice: Refer to Fastener Notice in the Preface section. Tighten 9 N·m (80 lb in)
2 | Charge Air Cooler