For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the charge air cooler outlet pipe from the intake manifold. Refer to Charge Air Cooler Outlet Pipe Replacement.

1 | Charge Air Bypass Valve Vacuum Tank Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the vacuum hoses.

Tighten
10 N·m (89 lb in)

2 | Charge Air Bypass Valve Vacuum Tank