For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Clutch Pedal Position Sensor Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Clutch Pedal Position Sensor

#### Procedures

1. Disconnect the clutch pedal position switch electrical connector.

Warning: Replacement or reprogramming of the ECM, or replacement of the clutch pedal position sensor (CPPS) or clutch pedal requires that a CPPS learn procedure be performed. Failure to perform the CPPS learn procedure may result in personal injury or damage to the vehicle or its components if the vehicle is in gear and the starter motor is accidentally engaged.

2. Perform the clutch pedal position sensor learn procedure. Refer to Clutch Pedal Position Sensor Learn for Getrag 5 speed transmission or Clutch Pedal Position Sensor Learn for MU3 transmission.