For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the headlamp assemblies. Refer to Headlamp Replacement.
2. Remove the front fender liners. Refer to Front Fender Liner Replacement.
3. Remove the front bumper air deflector. Refer to Front Bumper Fascia Air Deflector Replacement.
4. Remove the fog lamps, if equipped. Refer to Front Fog Lamp Replacement.

1 | Lower Front Bumper Fascia Plastic Retainer (Qty: 2)
2 | Front Bumper Fascia Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
3 | Upper Front Bumper Fascia Plastic Retainers (Qty: 4)
4 | Front Bumper Fascia

#### Procedure

Pull up on the front fascia to disconnect from the fender.